**Configuration**

End Device:

1. Open end device and go to Desktop -> IP Configuration
2. Set IP address, default gateway. Subnet mask is automatically filled.
3. Default gateway address is the address of the interface of the router connected to the network in which host is residing.

Router:

1. Before opening the router, see the interfaces by which the networks are connected. You can see the interface by placing your cursor on the red triangle displayed on link.
2. Open router, go to config -> the interface (fast Ethernet 0/0 or fast Ethernet 1/0). Set port status ON and give IP address of default gateway entered in the end device connected in the network.

